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PART 1 – GENERAL

1.01 SCOPE
A. SUPPLIER: Furnish and install Vertical Blinds (Premium Quality)
B. RELATED WORK SPECIFIED ELSEWHERE:
1. Section 06100: Rough Carpentry
2. Section 08520: Aluminum Windows
1.02 REFERENCES
A. FLAME-RESISTANT MATERIALS SHALL PASS OR EXCEED ONE OR MORE OF THE FOLLOWING TESTS:
· National Fire Protection Association (NFPA) 701 (small scale for horizontal applications)
· Department of Transportation Motor Vehicle Safety Standard 302 Flammability of Interior Materials
· California Administrative Code Title 19
· Federal Standard 191 Method 5903 (used by Port Authority of New York and New Jersey for drapery, curtain, and upholstery material)
· Boston Fire Department Test BFD IX-1
· New York State Uniform Fire Prevention and Building Code
1.03 SUBMITTALS
A. PRODUCT DATA: Manufacturer’s descriptive literature shall be submitted indicating materials, finishes, construction and installation instructions and verifying that product meets requirements specified. Manufacturers recommendations for maintenance and cleaning shall be included.
B. DRAWINGS AND DIAGRAMS: Wiring diagrams of any motorized components or units, working and assembly drawings shall be supplied as requested.   
C. SAMPLE: Responsible contracting officer or agent shall supply one sample shade of each type specified in this contract for approval. Supplied units shall be furnished complete with all required components, mounting and associated hardware, instructions, and warranty.
1.04 QUALITY ASSURANCE:
A. Supplier: Manufacturer, subsidiary or licensed agent shall be approved to supply the products specified, and to honor any claims against product presented in accordance with warranty.
B. INSTALLER: Installer or agent shall be qualified to install specified products by prior experience, demonstrated performance and acceptance of requirements of manufacturer, subsidiary, or licensed agent. Installer shall be responsible for an acceptable installation.
C. UNIFORMITY: Provide Vertical Blind of only one manufacturer for entire project. 
1.05 DELIVERY, STORAGE AND HANDLING:
A. Product shall be delivered to site in manufacturer’s original packaging.
B. Product shall be handled and stored to prevent damage to materials, finishes and operating mechanisms.
1.06 JOB CONDITIONS:
A. Prior to shade installation, building shall be enclosed.
B. Interior temperature shall be maintained between 60° F. and 90° F. during and after installation; relative humidity shall not exceed 80%. Wet work shall be complete and dry.
1.07 WARRANTY:
A. Lifetime Limited Warranty. Warranty limitations apply to vertical headrail, cord, & fabrics. Specific product warranties available from manufacturer or its authorized agent.

PART 2 – PRODUCTS

2.01 ACCEPTABLE MANUFACTURER
A. Hunter Douglas Architectural / 9900 Gidley St., El Monte,  CA 91731/ Phone: 800-727-8953 Fax: 800-205-9819/ Website: HDarchitectural.com, or architect approved equivalent.  
B. Product substitutions must be approved by architect minimum of 30 days prior to close of bid.
2.02 VERTICAL BLINDS
A. PRODUCT: Hunter Douglas “Contract Vertical Blind”
B. MATERIALS:
1. LOUVERS: Vinyl extruded from PVC 3 1/2” wide x (optional flat or S-Curve) with standard overlap of not less than 1/8”.  Finish with manufacturer’s standard colors selected by architect from manufacturer’s available contract colors. 
2. CHANNEL: Standard type sculpted headrail measuring 1.8” X 1” constructed of painted aluminum. Internally fit with an extruded aluminum tilt rod, engineered polymer carrier trucks, end caps and components required for specified performance and designed for smooth, quiet, trouble-free operation. 
3. CARRIER TRUCKS: Engineered polymer 0.3" thick and 1.3” wide with wheels and worm-and-spur gears to ensure rotation with perfect alignment and synchronization. Solid molded engineered thermal plastic asymmetrical carrier stems provide ease of louver installation and removal. 
4. ROTATION: Tilt wand provides180 degrees direct rotation by activating tilt gear within end cap assembly in turn actuating extruded aluminum tilt rod and worm-and-spur gears in carrier trucks. Located on either side of individual blind unit as per architect’s request. 
5. TRAVERSING: Stretch resistant, non-fraying, and lint free lock nit polyester cord provide traversing capabilities for side, center.
6. MOUNTING HARDWARE: Manufacturer’s standard L- bracket with clip (outside mounts) & clip only (inside mounts) provide required support. 
7. ADDITIONAL AVAILABLE OPTIONS: Valance, Wand Control, (Painted Aluminum) Headrail Systems.
2.03 FABRICATION
A. Blind measurements shall be accurate to within + 1/8” for width and +0/-¼" for height or as recommended in writing by manufacturer.
2.04 FINISHES
A. LOUVER finish selection from the following: (Vinyl Curved 3 ½”) White, Off-White, Ivory, Grey (Vinyl Flat 3 ½”) White, Off-White, Ivory, Grey, Brown

PART 3 - EXECUTION

3.01 INSPECTION:
A. SUBCONTRACTOR shall be responsible for inspection on site, approval of mounting surfaces, installation conditions and field measurement for this work.
B. OTHER INTERACTING TRADES shall receive drawings of shade systems, dimensions, assembly, and installation methods from subcontractor upon request.
3.02 INSTALLATION:
A. INSTALLATION shall comply with manufacturer’s specifications, standards and procedures as detailed on contract drawings.
B. ADEQUATE CLEARANCE shall be provided to permit unencumbered operation of shade and hardware.
C. CLEAN finish installation of dirt and finger marks. Leave work area clean and free of debris.
3.03 DEMONSTRATION:
A. Demonstrate operation method and instruct owner’s personnel in the proper operation and maintenance of the blinds.
3.04 SCHEDULE:
A. EXTERIOR WINDOWS:
B. INTERIOR RELIGHTS:
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